{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":112,"n_cols":8,"rows_kept":112,"merged":[[0,0,55,0],[0,3,5,3],[6,3,10,3],[11,3,15,3],[16,3,21,3],[22,3,23,3],[24,3,30,3],[31,3,37,3],[38,3,39,3],[40,2,41,2],[40,5,41,5],[42,2,43,2],[42,5,43,5],[44,2,45,2],[44,5,45,5],[46,2,47,2],[46,5,47,5],[48,2,49,2],[48,5,49,5],[50,2,51,2],[50,5,51,5],[52,2,53,2],[52,5,53,5],[54,2,55,2],[54,5,55,5],[56,0,111,0],[56,3,58,3],[59,3,60,3],[61,3,62,3],[63,3,64,3],[65,3,68,3],[69,3,70,3],[72,3,74,3],[75,3,79,3],[80,3,84,3],[85,3,86,3],[87,3,88,3],[89,3,90,3],[91,3,92,3],[96,2,97,2],[96,5,97,5],[98,2,99,2],[98,5,99,5],[100,2,101,2],[100,5,101,5],[102,2,103,2],[102,5,103,5],[104,2,105,2],[104,5,105,5],[106,2,107,2],[106,5,107,5],[108,2,109,2],[108,5,109,5],[110,2,111,2],[110,5,111,5]],"flags":["formulas_cached_only"]}
["主控板","A0","色质联用电流","继电控制板1","PE3","ADC0"]
[null,"A1","备用串口设备1电流控制口",null,"PE2","ADC1","48V转24V","输出高电平工作"]
[null,"A2","备用串口设备2电流控制口",null,"PE1","ADC2","48V转12V","输出低电平工作"]
[null,"A3","光通讯机电流",null,"PE0","ADC3"]
[null,"A4","ADCP电流",null,"PK0","ADC16"]
[null,"A5","CTD电流",null,"PK1","ADC17"]
[null,"A6","摄像1电流","继电控制板2","PK2","ADC18"]
[null,"A7","甲烷同位素分析仪电流",null,"PK3","ADC19"]
[null,"A8","ICL电流",null,"PB5","ADC11"]
[null,"A9","气相色谱仪电流",null,"PB4","ADC10"]
[null,"A10","二氧化碳电流",null,"PE4","ADC9"]
[null,"A11","显微拉曼分析仪电流","继电控制板3","PE5","ADC8"]
[null,"A12","质谱仪电流",null,"PD4","ADC7"]
[null,"A13","摄像2电流",null,"PD5","ADC6"]
[null,"A14","备用网口电流",null,"PD6","ADC5"]
[null,"A15","声学定位电流",null,"PD7","ADC4"]
[null,"Din1","色质联用输出反馈","继电控制板1","PM7"]
[null,"Din2","备用串口设备1输出反馈",null,"PM6"]
[null,"Din3","备用串口设备2输出反馈",null,"PM5"]
[null,"Din4","光通讯机输出反馈",null,"PM4"]
[null,"Din5","ADCP输出反馈",null,"PB2"]
[null,"Din6","CTD输出反馈",null,"PB3"]
[null,"Din7","摄像1输出反馈","继电控制板2","PL7"]
[null,"Din8","甲烷同位素分析仪输出反馈",null,"PL6"]
[null,"Dout1","色质联用输出控制口","继电控制板1","PN4"]
[null,"Dout2","备用串口设备1输出控制口",null,"PN3"]
[null,"Dout3","备用串口设备2输出控制口",null,"PN2"]
[null,"Dout4","光通讯机输出控制口",null,"PN1"]
[null,"Dout5","ADCP输出控制口",null,"PN0"]
[null,"Dout6","CTD输出控制口",null,"PP5"]
[null,"Dout7","反馈使能信号控制口",null,"PP4"]
[null,"Dout8","摄像1输出控制口","继电控制板2","PP3"]
[null,"Dout9","甲烷同位素分析仪输出控制口",null,"PL4"]
[null,"Dout10","ICL输出控制口",null,"PL3"]
[null,"Dout11","气相色谱仪输出控制口",null,"PL2"]
[null,"Dout12","二氧化碳输出控制口",null,"PL1"]
[null,"Dout13","工控机输出控制口",null,"PM0"]
[null,"Dout14","反馈信号控制口",null,"PM1"]
[null,"Dout15","显微拉曼分析仪输出控制口","继电控制板3","PM2"]
[null,"Dout16","质谱仪输出控制口",null,"PM3"]
[null,"串口0_RX","备用串口设备1",null,"PA0","串口0"]
[null,"串口0_TX",null,null,"PA1"]
[null,"串口1_RX","温湿度传感器",null,"PB0","串口1"]
[null,"串口1_TX",null,null,"PB1"]
[null,"串口2_RX","CTD",null,"PA6","串口2"]
[null,"串口2_TX",null,null,"PA7"]
[null,"串口3_RX","无",null,"PA4","串口3"]
[null,"串口3_TX",null,null,"PA5"]
[null,"串口4_RX","无",null,"PA2","串口4"]
[null,"串口4_TX",null,null,"PA3"]
[null,"串口5_RX","无",null,"PC6","串口5"]
[null,"串口5_TX",null,null,"PC7"]
[null,"串口6_RX","无",null,"PP0","串口6"]
[null,"串口6_TX",null,null,"PP1"]
[null,"串口7_RX","从控板通信",null,"PC4","串口7"]
[null,"串口7_TX",null,null,"PC5"]
["从板","A0","48V电压采样","电能转换板1","PE3","ADC0"]
[null,"A1","48V电流采样",null,"PE2","ADC1"]
[null,"A2","24V电流采样",null,"PE1","ADC2"]
[null,"A3","48V电流采样","电能转换板2","PE0","ADC3"]
[null,"A4","24V电流采样",null,"PK0","ADC16"]
[null,"A5","48V电流采样","电能转换板3","PK1","ADC17"]
[null,"A6","24V电流采样",null,"PK2","ADC18"]
[null,"A7","48V电流采样","电能转换板4","PK3","ADC19"]
[null,"A8","24V电流采样",null,"PB5","ADC11"]
[null,"A9","漏电流模块1","接地检测","PB4","ADC10"]
[null,"A10","漏电流模块2",null,"PE4","ADC9"]
[null,"A11","漏电流模块3",null,"PE5","ADC8"]
[null,"A12","漏电流模块4",null,"PD4","ADC7"]
[null,"A13","漏水检测1","漏水线缆","PD5","ADC6"]
[null,"A14","漏水检测2",null,"PD6","ADC5"]
[null,"A15","无",null,"PD7","ADC4"]
[null,"Din1","ICL输出反馈","继电控制板2","PM7"]
[null,"Din2","气相色谱仪输出反馈",null,"PM6"]
[null,"Din3","二氧化碳输出反馈",null,"PM5"]
[null,"Din4","显微拉曼输出反馈","继电控制板3","PM4"]
[null,"Din5","质谱仪输出反馈",null,"PB2"]
[null,"Din6","摄像2输出反馈",null,"PB3"]
[null,"Din7","备用网口输出反馈",null,"PL7"]
[null,"Din8","声学定位输出反馈",null,"PL6"]
[null,"Dout1","摄像2输出控制口","继电控制板3","PN4"]
[null,"Dout2","备用网口输出控制口",null,"PN3"]
[null,"Dout3","声学定位输出控制口",null,"PN2"]
[null,"Dout4","电交换机2控制口",null,"PN1"]
[null,"Dout5","反馈信号线控制口",null,"PN0"]
[null,"Dout6","24V电源模块控制口","电能转换板1","PP5"]
[null,"Dout7","12V电源模块控制口",null,"PP4"]
[null,"Dout8","24V电源模块控制口","电能转换板2","PP3"]
[null,"Dout9","12V电源模块控制口",null,"PL4"]
[null,"Dout10","24V电源模块控制口","电能转换板3","PL3"]
[null,"Dout11","12V电源模块控制口",null,"PL2"]
[null,"Dout12","24V电源模块控制口","电能转换板4","PL1"]
[null,"Dout13","12V电源模块控制口",null,"PM0"]
[null,"Dout14","无",null,"PM1"]
[null,"Dout15","无",null,"PM2"]
[null,"Dout16","无",null,"PM3"]
[null,"串口0_RX","工控机",null,"PA0","串口0"]
[null,"串口0_TX",null,null,"PA1"]
[null,"串口1_RX","温湿度传感器",null,"PB0","串口1"]
[null,"串口1_TX",null,null,"PB1"]
[null,"串口2_RX",null,null,"PA6","串口2"]
[null,"串口2_TX",null,null,"PA7"]
[null,"串口3_RX",null,null,"PA4","串口3"]
[null,"串口3_TX",null,null,"PA5"]
[null,"串口4_RX",null,null,"PA2","串口4"]
[null,"串口4_TX",null,null,"PA3"]
[null,"串口5_RX",null,null,"PC6","串口5"]
[null,"串口5_TX",null,null,"PC7"]
[null,"串口6_RX",null,null,"PP0","串口6"]
[null,"串口6_TX",null,null,"PP1"]
[null,"串口7_RX","从控板通信",null,"PC4","串口7"]
[null,"串口7_TX",null,null,"PC5"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}