{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":66,"n_cols":11,"rows_kept":66,"merged":[[2,0,3,0],[4,0,12,0],[13,0,22,0],[23,0,32,0],[33,0,42,0],[43,0,52,0],[53,0,61,0],[62,0,64,0],[65,0,66,10]],"flags":["formulas_cached_only"]}
["测试大类","测试小类","功能种类","各小类测试包含项","测试情况","遇到问题现象","问题时间","问题分析","解决方式","解决时间","解决情况"]
["时钟同步测试","时钟同步","任务书功能","1.验证上位机发送时间准确性","通过","无","无","无","无","无","无"]
["心跳包测试","周期性上传心跳包","任务书功能","2.验证周期上传的准确性","通过","无","无","无","无","无","无"]
[null,"设置心跳包上传的周期时间","非任务书功能","3.修改心跳上传的周期，并判断上传周期是否被修改","未通过","同步修改到配置文件中时，配置文件中含相同字段的地方都被修改","2022-10-18","字符串匹配的约束力不够，以及匹配方式存在严重bug","对程序中操作配置文件的标题判断进行了更多的约束","2022-10-18","已解决"]
["直流表测试","启动时周期性工作模式","任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时阶段性工作模式","非任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","未通过","部分时间进行配置时，一直发送数据，未阶段性的进行工作","2022-10-20","对未生效工作时间的判断使用了“与”判断，里应该是或判断","修改判断调条件","2022-10-20","已解决"]
[null,"启动时一直工作模式","非任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","数据一直没有发送","2022-10-19","之前对阶段性工作模式以及一直工作模式进行了文本保存的定时器添加，所以在进行模式切换时，里应该关闭该定时器，而实际上关闭了周期性模式工作的生效定时器","修改关闭的定时期ID","2022-10-19","已解决"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","同上","同上","同上","同上","同上","已解决"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
["多参数测试","启动时周期性工作模式","任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","未通过","数据上传异样","2022-10-18","多参数传感器具有开机启动时间，且开机启动时间大于手册的30S","每一次上电新增40S的启动延迟时间","2022-10-18","已解决"]
[null,"启动时阶段性工作模式","非任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时一直工作模式","非任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","数据没有发送","2022-10-19","由于多参数有电源控制，而在切换过程中没有添加电源控制","增加电源控制","2022-10-19","已解决"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","同上","同上","同上","同上","同上","已解决"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","同上","同上","同上","同上","同上","已解决"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","未通过","数据没有发送","2022-10-19","由于多参数有电源控制，而在切换过程中没有添加电源控制","增加电源控制","2022-10-19","已解决"]
[null,"通过上位机指令进行断电","任务书功能","1.上位机发送指令，进行断电，通过上传的数据进行判断","通过","无","无","无","无","无","无"]
["摄像机1","启动时周期性工作模式","非任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时阶段性工作模式","非任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时一直工作模式","任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"通过上位机指令进行断电","任务书功能","1.上位机发送指令，进行断电，通过上传的数据进行判断","通过","无","无","无","无","无","无"]
["摄像机2","启动时周期性工作模式","非任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时阶段性工作模式","非任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时一直工作模式","任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"通过上位机指令进行断电","任务书功能","1.上位机发送指令，进行断电，通过上传的数据进行判断","通过","无","无","无","无","无","无"]
["摄像灯","启动时周期性工作模式","非任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时阶段性工作模式","任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时一直工作模式","非任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"通过上位机指令进行断电","任务书功能","1.上位机发送指令，进行断电，通过上传的数据进行判断","通过","无","无","无","无","无","无"]
["温湿度","启动时周期性工作模式","任务书功能","1.根据预设的工作周期，工作时间，上传周期判定工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时阶段性工作模式","非任务书功能","1.根据设置的开始工作时间，结束工作时间，上传周期判断工作准确性\n2.可修改预设的工作周期，工作时间，上传周期，并同步到配置文件中","通过","无","无","无","无","无","无"]
[null,"启动时一直工作模式","非任务书功能","1.根据上传周期，判断工作的准确性。","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"周期性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转一直工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"阶段性工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转周期性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
[null,"一直工作模式转阶段性工作模式","非任务书功能","1.模式转换通过设置的各个参数进行现象判断","通过","无","无","无","无","无","无"]
["额外功能","远程重启","非任务书功能","1.上位机发送指令，看下位机运行灯判断是否重启","通过","无","无","无","无","无","无"]
[null,"远程升级","非任务书功能","1.上位机发送升级模式（带不带配置文件），根据内存卡上的bin文件进行判断","暂未测试"]
[null,"远程获取以及删除日志文件","非任务书功能","1.上位机获取文件，通过上位机保存日志文件的路径下是否存在文件进行判断\n2.下位机删除日志文件通过下位机保存日志文件判断","暂未测试"]
["注：添加功能：1.在一直工作模式以及阶段性工作模式中，新增工作时一小时保存一组数据。\n"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}